Power Transducer

|  | Catalog Edit :

Power Transducer

| Voltage Transducer VT95 Voltage Input 0-150 VAC, 0-300 VAC Analog Output 4-20 mA, 0-5 VDC, 0-10 VDC
| Voltage Transducer (3 phase) VT195 Input 3 Phase, 0-150 VAC,0-300 VAC Analog Output 4-20 mA, 0-5 VDC, 0-10 VDC
| Current Transducer CT95 Current Input 0-1 Aac, 0-5 Aac Analog Output 4-20 mA, 0-5 VDC, 0-10 VDC
| Current Transducer (3 phase) CT195 Current Input 0-1 Aac, 0-5 Aac Analog Output 4-20 mA, 0-5 VDC, 0-10 VDC
| Watt Transducer WAT95 Voltage Input 110 VAC, 220 VAC, 380 VAC Current Input 1 A, 5 A Analog Output 4-20 mA, 0-5 VDC
| Var Transducer VAR95 Voltage Input 110 VAC, 220 VAC, 380 VAC Current Input 1 A, 5 A Analog Output 4-20 mA, 0-5 VDC
| Frequency Transducer FQ95 Voltage Input 110 VAC, 220 VAC Analog Output 4-20 mA, 0-5 VDC, 0-10 VDC
| Current Transformer CT Rate Voltage: 660 VAC Output Capacity: 5 VA Max. Accuracy Class: 0.5