Accessories

|  | Catalog Edit :

Accessories

Forklift Speed Alarm
With LED Display Screen
Use Wireless Sensor
Two Kinds of Warning: Flash Lamp and Voice Alarm
External Powerful Horn for Alarm
Warning Sound Up to 120 db

| Power Supply DR-45-24 Output 24 VDC, 2 A Input 100 - 240 VAC DIN Rail Mounting
| Power Supply DR-120-24 Output 24 VDC, 5 A Input 100 to 240 VAC DIN Rail Mounting

Excite D.C. Supply
ES20
0 to 5 VDC or 0 to 10 Volts Output
50 mA Current Output
4 Channels Output
Supply to Load Cells or Strain Gauge etc.

| Current Transformer CT Rate Voltage: 660 VAC Output Capacity: 5 VA Max. Accuracy Class: 0.5

Pilot Lamp
PL2000
10 LED Lamp
3 Color Selectable
(Red, Blue, Green)
Programmable Flashing