Power Protective Relay

|  | Catalog Edit :

Power Protective Relay

Voltage Relay
VR95
ป้องกันแรงดันไฟฟ้าเกินหรือตก
สามารถตั้งหน่วงเวลาได้ 0 - 10 วินาที
มี LED แสดงสภาวะของ Relay
มี LED แสดงสภาวะแรงดันไฟฟ้าตกหรือเกิน

Voltage Relay
VR195
ป้องกันแรงดันไฟฟ้าเกินหรือตก
ช่วยลดความเสียหายของอุปกรณ์ไฟฟ้า
เนื่องจากแรงดันไฟฟ้าผิดปกติ
สามารถตั้งหน่วงเวลาได้ 0-10 วินาที
มี LED แสดงสภาวะแรงดันไฟฟ้าตกหรือเกิน

| Asymmetry Relay AR95 ป้องกันเฟสขาด, ต่อสลับเฟส ป้องกันแรงดันไฟฟ้าตกหรือเกิ

Current Relay
CR95
ป้องกันความเสียหายของ Motor และ Load
ป้องกันกระแสเกินหรือกระแสตก
ตั้งหน่วงเวลาได้ 0 -10 วินาที
ตั้งหน่วงเวลาขณะสตาร์ทได้ 0 - 30 วินาที
SPDT Relay Output

| Ground - Fault Relay ER95 ป้องกันกระแสรั่วลง Ground ตั้งหน่วงเวลาได้ 0 - 1 sec
| Insulation Monitoring Relay IR195 Insulation Monitor 10 to 200 KΩ SPDT Relay Contact Output. Earth Fault LED Indicator

Reverse Power Relay
RR20
Motoring protection
Adjustable time delay
Easy to install
Power signal output for indicator

Frequency Relay
FR95
Over-under frequency Protection
Output relay SPDT, 250V, 3A
LED indicate relay status
Signal output for panel meter display

| Speed Sensing Relay SS95 Magnetic pick-up input 3 Speed set point Output relay contact