4 Wire Transmitter

|  | Catalog Edit :

4-Wire Transmitter

| Universal Signal Conditioner SC20 Programmable Input mV, V, mA , Thermocouple, RTD Output 4-20 mA, 0-10 VDC, 1-5 VDC Isolated Input, Output and Power Supply
| Thermocouple Transmitter TT95 Input Thermocouple J, K, S, R, T Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC Isolated Input, Output and Power Supply

RTD Transmitter
RT95
TRD Transmitter
Input RTD PT100
Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC
Isolated Input, Output and Power Supply

| Potentiometer Transmitter PT95 Input Potentionmeter Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC Isolated Input, Output and Power Supply

Signal converter
SC95
Input 10 mV-100 VDC, 0-20 mA, 4-20 mA
Output 4-20 mA, 0-20 mA, 0-1 VDC, 0-5 VDC, 1-5 VDC,
0-10 VDC
Isolated Input, Output and Power Supply

| Frequency Transmitter FT20 Input Frequency 25 Hz 20 KHz Output 4-20 mA, 0-20 mA, 0-5 VDC, 1-5 VDC, 0-10 VDC Isolated Input, Output and Power Supply
| Weight Transmitter WT95 Input from Load Cell or Strain Guage Sensor Output 4-20 mA, 0-10 VDC, 1-5 VDC Adjustable Span and Tare
| Remote Setpoint RS95 Up - Dow Vary Setpoint Output 4-20 mA, 0-10 VDC, 0-5 VDC
| Digital Remote Setpoint RS20 Manual Adjust Output 4 to 20 mA, 0 to 10 VDC, 1 to 5 VDC Programmable Display
| Totalizer TL95 Convert Flow Rate to Totalizer Input 4-20 mA, 0-10 VDC, 1-5 VDC Output Frequency 25-51200 count/hour
| Square Root Transmitter ST20 Squared Input To Convert Diff Pressure to Flow Rate Input, Output 4-20 mA Isolated
| Peak-Hold Signal Conditioner SC21 Hold Maximum Value Signal 4-20 mA, 0-10 VDC, 1-5 VDC Isolated Input, Output and Power Supply
| High Selector HS95 Accept Two Input Signal Higher Selector DC Current 4 - 20 mA