2 Wire Transmitter

|  | Catalog Edit :

2-Wire Transmitter

2-Wire Programmable Transmitter
SC23
1 Input, 1 Output
Programmable Input
Output 2 Wire 4-20 mA (Loop Power)
Isolated Input/Output and Power Supply

2-Wire Programmable Transmitter
SC24
2 Input, 2 Output
Programmable Input
Output 2 Wire 4-20 mA (Loop Power)
Isolated Input/Output and Power Supply

2-Wire Programmable Transmitter
SC25
1 Input, 2 Output
Programmable Input
Output 2 Wire 4-20 mA (Loop Power)
Isolated Input/Output and Power Supply

| Temperature Transmitter TR37 High Accuracy Temperature ± 0.1 °C Temperature Range 0 - 100 °C Output 2 Wire 4-20 mA (Loop Power)
| Humidity Transmitter HR370 Precision Relative Humidity ± 3 % RH Humidity Range 0 - 100 % RH Output 2 Wire 4 - 20 mA (Loop Powered)
| RTD Transmitter (PT100) RT37 Input RTD PT100 Output 2 Wire 4-20 mA (Loop Power) Isolated input to output
| Thermocouple Transmitter TT37 Input Thermocouple J, K, S, R, T Output 2 Wire 4-20 mA (Loop Power) Isolated input to output
| Potentiometer Transmitter PT37 Input Potentionmeter 100 Ω to 50 KΩ Output 2 Wire 4-20 mA (Loop Power) Isolated input to output
| Current Transmitter CT37 Input 0-1, 0-5 A (AC) Output 2 Wire 4-20 mA (Loop Power) Isolated input to output
| Signal Converter SC37 Input 10 mVDC to 100 VDC, 100 µADC to 100 mADC Output 2 Wire 4-20 mA (Loop Power) Isolated input to output
| P/I Signal Converter PC37 Input 0.2 to 1 Bar, 3 to 15 PSI Output 2 Wire 4-20 mA (Loop Power) Isolated input to output
| Differential Pressure DT20 Input Pressure 5 inch W.G. to 1 Bar Output 2 Wire 4-20 mA (Loop Powered)

Pressure Transmitter
DT21
Piezoresistive silicon chip employed Resolution
Perfect long term stability
MEMS technology
CE certificate

| Level Transmitter LT20 วัดระดับของเหลว Output 4-20 mA Easy Install
| Humidity Transmitter HT120 Precision Relative Humidity ± 3 % RH High Accuracy Temperature ± 0.4 °C Output 2 Wire 4-20 mA (Loop Powered)

Humidity Transmitter
HT130
Working Range (-)40 to 125 °C
Precision Relative Humidity ± 3 % RH
High Accuracy Temperature ± 0.4 °C
Output 2 Wire 4-20 mA (Loop Powered)

Current Loop Supply
(2 channels distributer)
CS295
Power supply for 2 wire transmitter
Supplies 2 Current Loops
Isolation between each Current Loop and power supply
Current limiting (short circuit protected)

Current Loop Supply
(Isolated distributer)
CS195
Power 2 Wire Transmitter
Output 4-20 mA, 1-5 VDC, 0-10 VDC
Isolated between input, output and supply

Current Loop Supply
(Isolated 2 Output)
CS198
Power 2 Wire Transmitter
2 Channels Output 4-20 mA, 1-5 VDC, 0-10 VDC
Isolated between input, output and supply

Current Loop Supply
CS20
Power Supply for 2-wire Transmitter
Supplies 8 Current Loops
Current Limiting
Short Circuit Protected (Relay Alarm)

Signal Isolater
SI99
Intrinsically safe isolation without power supply
Eliminating ground-loop
2 channels available
High accuracy and stability