Data Acquisition, MODBUS I/O Module (RS-232, RS-485)

|  | Catalog Edit :

Data Acquisition, MODBUS I/O Module
(RS-232, RS-485)

| Universal Analog Input Module AI20 Programmable Input Type 1 Analog Input Channel RS-485 Isolated

Analog Input Module
AI210
Programmable Input Type
8 Analog Input Channels
4 Digital Input Channels
4 Digital Output Channels
RS-232, RS-485 Isolated

| Expansion Module EX24 Programmable Input Type 16 Analog Input Channels DIN Rail Mounting

Analog Input Module
AI250
4 Programable Analog Input
2 Digital Input, 2 Counter
2 Digital Output
MODBUS TCP/IP

| Analog Output Module AO200 4 Channels Output Isolated Output 4-20 mA, 0-10 VDC, 1-5 VDC RS232, RS485 Isolated

Digital Input Module
DI100
32 Digital Input (Opto Isolated)
RS485 Isolated
MODBUS Protocol
DIN Rail Mounting

Digital Input Module
DI2000
32 Digital Input (Opto Isolated)
RS232, RS485 Isolated
MODBUS Protocol
DIN Rail Mounting

| Digital Input/Output Module DIO100 16 Digital Input (Isolated 1000 V) 8 Digital Output (Relay Contact) RS485 Isolated
| Digital Input/Output Module DIO2100 16 Digital Input (Isolated 1000 V) 8 Digital Output (Relay Contact) RS485 Isolated

Digital Counter Module
DC2100
16 Digital Input Channels
Channel 1-8 can be Programmable (Status, Counter,
Frequency)
Support Protocol MODBUS RTU or ASCII Command
Support Quadrature Counter, Frequency (Hz) Mode

| Digital Output Module DO100 16 Digital Output (Relay Contact) Protocol MODBUS or ASCII Command RS232, RS485 Isolated (1000 V)
| Digital Output Module DO2000 16 Digital Output (Relay Contact) Protocol MODBUS or ASCII Command RS232, RS485 Isolated (1000 V)
| Digital Remote Display DP23 7-Segment LED Display 8 Digits Display Controlled by MODBUS Protocol (RS-485)
| Digital Remote Display DP24 7-Segment LED Display 4 Digits Display Controlled by MODBUS Protocol (RS-485)

Big Digital Remote Display
DP60
7-Segment LED Display
6 Digits Display
100 mm. Height
Controlled by MODBUS Protocol (RS-485)

Big Digital Remote Display
DP61
7-Segment LED Display
6 Digits Display 100 mm.
Ethernet LAN / WiFi Connection
MODBUS TCP/IP Protocol

Humidity & Temperature
To RS485 (Modbus)
HT20
1 Humidity Channel
1 Temperature Channel
1 Dew Point Channel
Communication Modbus Protocol ASCII and RTU

Humidity & Temperature
HT21
2 Rows LCD Display
1 Humidity Channel
1 Temperature Channel
1 Dew Point Channel
Communication Modbus Protocol ASCII and RTU

| Temperature To RS485 (Modbus) TR38 1 Temperature Channel Temperature Range (-)20 to 100 °C Communication Modbus Protocol ASCII and RTU

3G Modbus Data Center
RC51
Automatic Synchronous Database Server
Built-in 3G Modem (UMTS/HSDPA)
Online Monitoring
Easy Setting by Embedded Web Console
Keep Data as Tag (Max. 128 tags Option)
Support Modbus RTU, ASCII ,TCP
Data backup more than 1 Week

Modbus Data Center
RC52
Automatic Synchronous Database Server
Interface RS-232, RS-485/422
Online Monitoring
Easy Setting by Embedded Web Console
Keep Data as Tag (Max. 128 tags Option)
Support Modbus RTU, ASCII ,TCP
Data backup more than 1 Week

Modbus Gateway
RC32
Convert between Modbus TCP and Modbus RTU/ASCII
1 Ethernet port and 1 RS-232, RS422/485 ports
Supports 8 simultaneous TCP masters with up to 32 simultaneous requests per master
Easy hardware setup and configurationy

| Multifunction Power Meter JYS-9Y4 Display V, I, Hz, PF, W, Var, Va, Kwh, Kvarh Pulse Output RS-485 Modbus Communication

Pilot Lamp (MODBUS)
PL2100
10 LED Lamps
7 Color Selectable
Programmable Flashing
Interface RS485
Support MODBUS RTU, ASCII

Pilot Lamp (MODBUS TCP/IP)
PL2200
10 LED Lamps
7 Color Selectable
Programmable Flashing
Interface RJ45
Support MODBUS TCP/IP

Modbus Remote Switch
RS2100
7 Color Selectable
Programmable Flashing
Interface RS485
Support MODBUS RTU, ASCII