Data Logger

|  | Catalog Edit :

Data Logger

PC - Based Recorder
AI210
Programmable Input Type
8 Analog Input Channels
4 Digital Input Channels
4 Digital Output Channels
RS-232, RS-485 Isolated

Wireless Data Logger
8 Channels Expandable to 768 Channels
Programmable Input Type
8 Analog Input Channels up to 768 Channels
RS-232, RS-485 Isolated
No Wiring (RF Link)

Data Logger
DL2200
8 Channels Analog Input (Programmable input)
24 Channels Analog Input เมื่อเพิ่ม Module EX24
4 Channels Digital Input/Output
Isolation Analog Input with Relay, Digital Input with Optoelectronic
Easily configure at Panel LCD and Keyboard
Use SD card memory for Data Storage (4GB)
Stand Alone Data Logger and Real Time Data Acquisition

| Data Logger ML21 1 Channel Analog Input (4-20 mA, 0-5 VDC, 0-10 VDC) Memory 64 Kbyte (Up to 256 Kbyte) Data exportable to MS Excel

Data Logger
ML22
2 Channels Analog Input (4-20mA, 0-100 mV, 0-200 mV, 0-1 V, 0-5 V)
High-speed Record Mode (Interval 5 msecs)
Memory 128 Kbyte (Up to 256 Kbyte)
Data exportable to MS Excel

| Data Logger ML24 2 Channels Temperature Input (RTD Pt100) Memory 128 Kbyte Data exportable to MS Excel
| Data Logger ML25 3 Channels A.C. Current Memory 64 Kbyte (Up to 256 Kbyte) Data exportable to MS Excel

Data Logger
(Humidity & High Temperature)
ML27
1 Channel Humidity
1 Channel Temperature
Memory 64 Kbyte (Up to 256 Kbyte)
Data exportable to MS Excel

Even Datalogger
ML28
4 Channels Digital Input
ON/OFF Time Stamp
Memory 128 Kbyte
Data exportable to MS Excel

Data Logger
(Humidity & High Temperature)
ML29
2 Channels
Humidity & Temperature
Memory 64 Kbyte (Up to 256 Kbyte)
Data Exportable to Excel, Access

Data Logger
CL23
1 Channel Analog Input (4-20 mA, 0-10 VDC)
2 Channels Totalizer
Memory 64 Kbyte (Up to 256 Kbyte)
Data exportable to MS Excel

Data Logger
CL24
1 Channel Analog Input (4-20 mA, 0-10 VDC)
2 Channels Totalizer
Memory 256 KByte
Data exportable to MS Excel

GPRS Data Logger
CL27
Smart Phone, Tablet, PC. Real Time Monitoring
4 Channels Analog Input
2 Channels Totalizer
GPRS Data Transfer
Centralize data logger (Logger on common database)
Flash memory 8 MByte
SMS Alarm (Send alarm to defined number)
Two Relay Output Control VIA SMS

Ethernet Data Logger
CL28
Smart Phone, Tablet, PC. Real Time Monitoring
4 Channels Analog Input
2 Channels Totalizer
Ethernet Data Transfer
Centralize data logger (Logger on common database) Flash memory 1 MByte

3G Data Logger
CL32
Smart Phone, Tablet, PC. Real Time Monitoring
4 Analog Input
2 Digital Input (Logic or Counter)
Built-in 3G Modem (UMTS/HSDPA)
Centralize data logger (Logger on common Database)
Support External Supply

3G Modbus Data Center
RC51
Smart Phone, Tablet, PC. Real Time Monitoring
Automatic Synchronous Database Server
Built-in 3G Modem (UMTS/HSDPA)
Easy Setting by Embedded Web Console
Keep Data as Tag (Max. 128 tags Option)
Support Modbus RTU, ASCII ,TCP
Data backup more than 1 Week

Modbus Data Center
RC52
Smart Phone, Tablet, PC. Real Time Monitoring
Automatic Synchronous Database Server
Interface RS232, RS485/422
Easy Setting by Embedded Web Console
Keep Data as Tag (Max. 128 tags Option)
Support Modbus RTU, ASCII ,TCP
Data backup more than 1 Week

Modbus Data Logger
RC53
Keep Data as Tag Max. 80 Tags (128 Tags Option)
Keep Record in csv File Format (Excel)
Remappable Modbus Register Address
Provides Modbus TCP Server
Support Micro SD Card up to 32 GB.