Data Communications

|  | Catalog Edit :

Data Communications

Modbus Gateway
MC320
Convert Between Modbus TCP/IP and Modbus RTU/ASCII
1 Ethernet Port and 1 RS232/RS422/485 Ports
Supports 8 TCP/IP MODBUS Protocol Device and 32 MODBUS Serial Connection
Easy Hardware Setup and Configuration

Modbus Gateway
RC32
Convert between Modbus TCP and Modbus RTU/ASCII
1 Ethernet port and 1 RS-232, RS422/485 ports
Supports 8 simultaneous TCP masters with up to 32 simultaneous requests per master
Easy hardware setup and configuration

Serial to Ethernet Converter
MC330
Communicate Serial Device Over Ethernet
Simultaneously Connect 4 Ethernet Device
Extend Serial Connection Distance
Bundle Virtual Serial Port Emulator

RS-232/RS-485/RS-422
Ethernet Converter
RC33
Control Serial Device over Ethernet
10/100 Mbps Ethernet Interface
Distance Serial Connections

Serial to 4G LTE Converter
MC331
Control Serial Device Over 4G (LTE)
Built-in 4G Modem
Simultaneously 4 Connect Device
Extend Serial Connection Distance
Serial Interface Compatible RS232/485/422

USB to RS-232/RS-485 Converter
RC22
RS-485 (2-Wire)
115.2 kbps Data Rate
Opto Isolation
Internal Power Supply

USB to Serial Converter
(RS485/RS422)
MC200
RS485 (2-Wire)
2 Channels
115.2 kbps Data Rate
Opto Isolation
Internal Power Supply

RS-232 to RS-485/RS-422 Converter
RC23
2-Wire / 4-Wire Operation
115.2 kbps Data Rate
Opto Isolation
Built-In Power Supply

| RS-485/RS422 Repeater RP23 Extend RS-485/RS-422 Distance 115.2 kbps Data Rate Galvanic Isolation
| RS485 Repeater RP24 Extend RS485 Distance 115.2 kbps Data Rate Galvanic Isolation

RS-232 Optical Isolator
RP22
Lighting Surges Protection
115.2 kbps Data Rate
2500 VAC Isolation
DB9 Connection

GSM ALARM
RC37
8 Alarm Digital inputs
Programmable SMS Message
2 Digital Output Controlled by SMS
Built-in 3G Modem (UMTS/HSDPA)

GSM ALARM
RC38
4 Analog Channels High-Low Alarm
2 Digital (Counter or Status) Alarm
Programmable SMS Message
Two Relay Output Control VIA SMS
Read Out VIA SMS
Built-in 3G Modem (UMTS/HSDPA)

| USB to RS-232 Converter RC27 115.2 kbps Data Rate Internal Power Supply

3G Modbus Data Center
RC51
Smart Phone, Tablet, PC. Real Time Monitoring
Automatic Synchronous Database Server
Built-in 3G Modem (UMTS/HSDPA)
Easy Setting by Embedded Web Console
Keep Data as Tag (Max. 128 tags Option)
Support Modbus RTU, ASCII ,TCP
Data backup more than 1 Week

Modbus Data Center
RC52
Smart Phone, Tablet, PC. Real Time Monitoring
Automatic Synchronous Database Server
Interface RS-232, RS-485/422
Easy Setting by Embedded Web Console
Keep Data as Tag (Max. 128 tags Option)
Support Modbus RTU, ASCII ,TCP
Data backup more than 1 Week

| Wireless RS232/485/422 RC35 Long Distance 700 m. No Wiring (RF Link) Easy to install
| Wireless RS485/422 RC36 Long Distance 700 m. No Wiring (RF Link) Easy to install
| Radio Modem RC45 Long Distance 700 m. No Wiring (RF Link) Easy to install

USB Isolator
RC43A
Supports USB 1.1 and 2.0 Compatible
2.5 KV Isolated
USB Standard Type A
No external power supply required
No software or drivers required