4 Wire Transmitter (2 Outputs)

|  | Catalog Edit :

4-Wire Transmitter (2 Outputs)

| Universal Signal Conditioner SC22 Programmable Input mA, mV, VDC, Thermocouple, RTD Two Isolated Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC Isolated Input, Output and Power Supply
| Thermocouple Transmitter TT98 Input Thermocouple K, J, L, R, S, T Two Isolated Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC Isolated Input, Output and Power Supply
| RTD Transmitter RT98 Input RTD PT100 Two Isolated Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC Isolated Input, Output and Power Supply
| Potentiometer Transmitter PT98 Input Potentionmeter 100 Ω to 50 KΩ Two Isolated Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC Isolated Input, Output and Power Supply

Signal converter
SC98
Input 10 mVDC to 100 VDC, 4-20 mA, 0-20 mA, 0-10 VDC,
1-5 VDC
Two Isolated Output 4-20 mA, 0-10 VDC, 0-5 VDC, 1-5 VDC
Isolated Input, Output and Power Supply

Signal Converter 2 Channels
SC99
Input 10 mVDC to 100 VDC, 4-20 mA, 0-20 mA, 0-10 VDC,
1-5 VDC
Two Channels input-output separated 4-20 mA, 0-10 VDC,
0-5 VDC, 1-5 VDC
Isolated Input, Output and Power Supply