Digital Panelmeter

|  | Catalog Edit :

Digital Panelmeter

Universal Input Indicator
DP70
5 Digits LED Display
Programmable Input (mA, mV, V, TC, RTD)
2 Alarm Relay
1 Analog Output or RS-485 (Optional)

| Digital Process Indicator DP20 3 ½ Digits LED Display Input 4-20 mA, 1-5 VDC, 0-5 VDC, 0-10 VDC Adjustable Display Scaling
| Loop Power Indicator DP32 Input 4 - 20 mA Looped Power (No Aux. Supply) Programmable Display
| Temperature Indicator TI20 3 ½ Digits LED Display Input Thermocouple or PT100 With 4-20 mA, 0-10 VDC Output (Optional)
| Digital Process Indicator DP95 3 ½ Digits LED Display Input 4-20 mA, 1-5 VDC, 0-5 VDC, 0-10 VDC Two Alarm Relay Output
| Temperature Indicator TI95 3 ½ Digits LED Diplay Input Thermocouple or PT100 Two Alarm Relay Output

Digital Counter Indicator
DP41
6 Digit Counter
Programmable Scaling
RS485 Modbus Communication
Bi-Direction Control

| Ratemeter & Totalizer DP21 8 Digits Display Programmable Scale Display Flow Rate and Totalizer
| Digital Tachometer (RPM/Hz) DP22 Large 4 Digits Display Display RPM or Hz. Input from Proximity Switch

Differential Pressure Controller
DP31
4 Digitals Display
Clean Room Monitoring
Air Filter Monitoring
2 Alarm With Relay Output

| Digital Remote Display DP23 7-Segment LED Display 8 Digits Display Controlled by MODBUS Protocol (RS-485)
| Digital Remote Display DP24 7-Segment LED Display 4 Digits Display Controlled by MODBUS Protocol (RS-485)