PLC Analog Input-Output

|  | Catalog Edit :

PLC Analog Input-Output

Thermocouple To Frequency
TF96
Interface to PLC digital input
Programmable range
Linearized output
Isolation of input, output and power supply
Cold junction compensation

RTD To Frequency
RF96
Interface to PLC digital input
Programmable Range
Isolated input to output to Power supply
True lead length compensation

DC To Frequency
DF96
Interface to PLC digital input
Programmable Range
Linearized output
Isolated input to output to Power supply
D.C. input voltage or current

Potentiometer To Frequency
PF96
Interface to PLC digital input
Sense position of potentiometer
Linearized output
Isolation between input, Output and power supply

| D To A Converter DA98 8 bit D to A converter Isolated input, output PLC analog Output