Touch Screen

|  | Catalog Edit :

Touch Screen

Alarm Indicator
AL32
Monitor 32 Alarm Inputs Max.
With Alarm Annunciator
Record Alarm Time in SD Card
2-Wire RS485 Wiring

Alarm Indicator
AL64
Monitor 32 Alarm Inputs Max.
With Alarm Annunciator
Record Alarm Time in SD Card
2-Wire RS485 Wiring

| Machine Monitor and Record MM32 Monitor Status of 32 Machine Max. Record Run Time in SD Card 2-Wire RS485 Wiring
| Tower Light Indicator TL10 Monitor 10 Tower Light Status Record Status Data in SD Card 2-Wire RS485 Wiring
| Tower Light Indicator TL20 Monitor 20 Tower Light Status Record Status Data in SD Card 2-Wire RS485 Wiring
| Remote Switch RS16 Control ON-OFF 16 Switch Max. Record ON-OFF Time in SD Card 2-Wire RS485 Wiring
| Remote Switch RS32 Control ON-OFF 32 Switch Max. Record ON-OFF Time in SD Card 2-Wire RS485 Wiring