Alarm Module

|  | Catalog Edit :

Alarm Module

Notify Alarm System AL100
AL100
24 Alarm Digital Inputs
Sending Alarm to LINE Notify, E-Mail
Programmable Alarm Message
Buffer 100 Alarm Message (Network Fail)
Support Passive POE

DC Alarm
DA95
Two alarm set points
DC. current or voltage input (4-20 mA, 1-5 VDC, 0-10 VDC)
SPDT relay output
24 VDC supply for 2-wire transmitter

| Thermistor Trip Relay TM495 ป้องกัน Motor หรือ Transformer เสียหาย เนื่องจากอุณหภูมิสูง PTC Thermistor Sensor Sensor Fail Detection
| Thermistor Trip Relay TM395 Prevent Motor/Transformer damage from high-temp PTC Thermistor Sensor Two Level Protection (Alarm and Trip)

Alarm Annunciator
AL1000
10 Channels Input
Siren Relay Output
First Alarm Detect
Expandable Input Channel

Alarm Annunciator
AL2000
10 Channels Input
LED Display
Siren Relay Output
First Alarm Detect
Expandable Input Channel

Alarm Annunciator
AL3000
10 Channels Input
LED Display
Siren Relay Output
First Alarm Detect
Expandable Input Channel

Pilot Lamp
PL2000
10 LED Lamp
3 Color Selectable
(Red, Blue, Green)
Programmable Flashing

GSM ALARM
RC37
8 Alarm Digital inputs
Programmable SMS Message
2 Digital Output Controlled by SMS
900, 1800 GSM Networks

GSM ALARM
RC38
4 Analog Channels High-Low Alarm
2 Digital (Counter or Status) Alarm
Programmable SMS Message
Two Relay Output Control VIA SMS
Read Out VIA SMS